**Europe Region dial pattern**

Norwegian User dial Pattern

Norwegian user should be follow the below dial patter from Jabber.

|  |  |
| --- | --- |
| **Description** | **Dialling pattern format** |
| UK Internal dial | 16<Last 5 digit of directory number> |
| Norway Internal dial | 35<Last 5 digit of directory number> |
| America Internal dial | 30<Last 5 digit of directory number> |
| Asia Internal Dial | 61<Last 5 digit of directory number> |
| India Internal call | 71<Last 5 digit of directory number> |
| External Norway number | 0<8 digit Norway number> |
| International calling | 000<country code><Phone number> |
| Service Desk | 70000 |

Aberdeen User Dial Pattern

Aberdeen user should be follow the below dial format from Jabber

|  |  |
| --- | --- |
| **Description** | **Dialling pattern format** |
| UK Internal dial | 16<Last 5 digit of directory number> |
| Norway Internal dial | 35<Last 5 digit of directory number> |
| America Internal dial | 30<Last 5 digit of directory number> |
| Asia Internal Dial | 61<Last 5 digit of directory number> |
| India Internal call | 71<Last 5 digit of directory number> |
| External UK number | 90<External number> |
| International calling | 900<country code><Phone number> |
| Service Desk | 70000 |

Chiswick User Dial Pattern

Chiswick user should be follow the below dial format from Jabber

|  |  |
| --- | --- |
| **Description** | **Dialling pattern format** |
| UK Internal dial | 16<Last 5 digit of directory number> |
| Norway Internal dial | 35<Last 5 digit of directory number> |
| America Internal dial | 30<Last 5 digit of directory number> |
| Asia Internal Dial | 61<Last 5 digit of directory number> |
| India Internal call | 71<Last 5 digit of directory number> |
| National call | 90<External number> |
| UK Internal dial | +44<Phone number> |
| International calling | 900<country code><Phone number> |
| Service Desk | 70000 |

Winnersh User Dial Pattern

Winnersh user should be follow the below dial format from Jabber

|  |  |
| --- | --- |
| **Winnersh** |  |
| **Description** | **Dialling pattern format** |
| UK Internal dial | 16<Last 5 digit of directory number> |
| Norway Internal dial | 35<Last 5 digit of directory number> |
| America Internal dial | 30<Last 5 digit of directory number> |
| Asia Internal Dial | 61<Last 5 digit of directory number> |
| India Internal call | 71<Last 5 digit of directory number> |
| National call | 90<External number> |
| UK National dial | "+44<Phone number> |
| International calling | 900<country code><Phone number> |
| Service Desk | 70000 |

|  |  |
| --- | --- |
| **Angola** |  |
| **Description** | **Dialling pattern format** |
| UK Internal dial | 16<Last 5 digit of directory number> |
| Norway Internal dial | 35<Last 5 digit of directory number> |
| America Internal dial | 30<Last 5 digit of directory number> |
| Asia Internal Dial | 61<Last 5 digit of directory number> |
| India Internal call | 71<Last 5 digit of directory number> |
| External Angola number | 0<Angola phone number> |
| International calling | 000<country code><Phone number> |
| Service Desk | 70000 |

**US Region dial pattern**

America BPI and Mobile dial Pattern

|  |  |
| --- | --- |
| **Description** | **Dialling pattern format** |
| UK Internal dial | 16<Last 5 digit of directory number> |
| Norway Internal dial | 35<Last 5 digit of directory number> |
| America Internal dial | 30<Last 5 digit of directory number> |
| Asia Internal Dial | 61<Last 5 digit of directory number> |
| India Internal call | 71<Last 5 digit of directory number> |
| Local dialling Amarica 7 digit | 00<7 digit number> |
| Long distance Amarica | 001<Phone number> |
| International calling | 00011<country code><Phone number> |
| Service Desk | 70000 |

Brazil - Curtiba, RDO, RIO and Macae dial Pattern

|  |  |
| --- | --- |
| **Description** | **Dialling pattern format** |
| UK Internal dial | 16<Last 5 digit of directory number> |
| Norway Internal dial | 35<Last 5 digit of directory number> |
| America Internal dial | 30<Last 5 digit of directory number> |
| Asia Internal Dial | 61<Last 5 digit of directory number> |
| India Internal call | 71<Last 5 digit of directory number> |
| Local number dialling | 00<Phone number> |
| National Number dialling | 000<Phone number> |
| International calling | 0000<country code><Phone number> |
| Service Desk | 70000 |

**APAC Region dial pattern**

Malaysia user dial pattern

|  |  |
| --- | --- |
| **Description** | **Dialling pattern format** |
| UK Internal dial | 16<Last 5 digit of directory number> |
| Norway Internal dial | 35<Last 5 digit of directory number> |
| America Internal dial | 30<Last 5 digit of directory number> |
| Asia Internal Dial | 61<Last 5 digit of directory number> |
| India Internal call | 71<Last 5 digit of directory number> |
| Local number dialling Asia | 00<Phone number> |
| Malaysiya local Number dialling | 000<Phone number> |
| International calling | 0000<country code><Phone number> |
| Service Desk | 70000 |

Brunei user dial pattern

|  |  |
| --- | --- |
| **Description** | **Dialling pattern format** |
| UK Internal dial | 16<Last 5 digit of directory number> |
| Norway Internal dial | 35<Last 5 digit of directory number> |
| America Internal dial | 30<Last 5 digit of directory number> |
| Asia Internal Dial | 61<Last 5 digit of directory number> |
| India Internal call | 71<Last 5 digit of directory number> |
| External Brunei number | 00<Brunei phone number> |
| International calling | 0000<country code><Phone number> |
| Service Desk | 70000 |